                           Supplement to S12 – free form


EVACUATION PROCEDURES

Vessel may be evacuated if a bomb threat or imminent danger to the vessel and/or terminal exists.

Guidance may be given by the PFSO/ National Authority to evacuate and the Master must take this into account when considering evacuation.

Evacuation may be partial (i.e. non-essential personnel will be evacuated) or full. Verbal instructions will be given accordingly.

Evacuation must be done in a controlled manner similar to that of abandoning ship. On the verbal order of the Master of the vessel to evacuate the vessel crew, visitors and passengers (if applicable) must muster, using the outside ladders of the deck house as follows -
1) Main deck if evacuation is by gangway or ladder to the jetty 

or helicopter.

2) Appropriate (order will be given) lifeboat muster station.

Note: In some circumstances evacuation to shore may preclude mustering on board due to urgency. In this case mustering of personnel is to be made ashore (Visitors log to be taken ashore to check visitor mustering). 

After completion of mustering the personnel will be counted and proceed to -

1) Shore gangway/ accommodation ladder – if evacuation via the shore. 

In some cases (extreme measures) the Master may consider evacuation via pilot ladder or the lifeboat (where applicable) /life raft embarkation ladders.


2) Lifeboat – if evacuation by lifeboat.

3) Helicopter winching area– if evacuation by winching into a helicopter.
Notes: 

a) Elevator should not to be used during evacuation (where fitted)

b) Drill and exercise scenario S13 for Vessel Evacuation forms part of this procedure as well as S14 Drill and exercise log sheet. 
