S10 – SECURITY MONITORING OF DECK & ADJACENT AREAS
(WATERSIDE & QUAYSIDE – see also S3 and S5 for monitoring information)

Ship’s Name:


	
	Level 1
	Level 2
	Level 3
	Remarks

	Deck areas
	1. Monitored visually
2.  Monitored by camera (C1)
3.  Covered by security lighting

	1.   Monitored visually
2.  Monitored by camera (C1)
3.  Covered by security lighting

4. Checked at intervals by security patrol
	1. Monitored visually
2. Monitored by camera (C1)
3. Covered by security lighting

4. Checked at intervals by security patrol
	Security patrol to be carried out with torch, whistle and radio communication with OOW. Patrol to be doubled at level 3 if felt necessary.

	Waterside
	1. Monitored visually
2.  Monitored by camera (C1)
3.   Covered by security lighting
	1.   Monitored visually

2.  Monitored by camera (C1)
3. Covered by security lighting

4.   Establish restricted area around ship

5.   Checked at intervals by security patrol boat
	1.   Monitored visually
2.  Monitored by camera (C1)
3.   Covered by security lighting

4.   Establish restricted area around ship

5.   Continuous presence of security patrol boat


	Security patrol to be carried out with torch, whistle and radio communication with OOW.
Patrol to be doubled at level 3 if felt necessary.

Level 3 – Port Security patrol may be provided by port security facilities. Comply with instructions issued by those responding to the security threat. Co-operate with the port facility and make preparations for underwater inspection of the hull / consider starting (if practical) or turning the main engine to deter underwater access. 

	Quayside
	1. Monitored visually
2.  Monitored by camera (C1)
3.   Covered by security lighting
	1.   Monitored visually
2.  Monitored by camera (C1)
3.   Covered by security lighting

4.   Establish restricted area around ship

5.   Checked at intervals by security patrol
	1.   Monitored visually
2.  Monitored by camera (C1)
3.   Covered by security lighting

4.   Establish restricted area around ship

5.   Continuous presence of security patrol
	Patrol to be doubled at level 3 if felt necessary.

Secure area on quayside is to be in co-operation with the PFSO.

If vessels freeboard allows easy access from the jetty then additional monitoring/ lighting is to be arranged according to the degree of risk. 


Note: Identification Check point near Gangway is to be properly illuminated. 
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