S25 – DURING TRANSIT OF GULF OF ADEN OR HIGH RISK AREA CHECKLIST

	
	Item
	Masters comments

	1
	All Doors to all Stores will be kept shut and locked throughout the transit.
	

	2
	No work outside the accommodation from arrival the entry point until:
	

	3
	All lights to be blinded off. No light out of accommodation.
	

	4
	Fire pump running and hoses pressurised discharged overside:
	

	5
	Accommodation secured all decks and Engine room entrances - by ddhhmm
	

	6
	No Engine maintenance on Fire P/P’s generators, steering etc.
	

	7
	No running of any cargo equipment, from before transit until well clear.
	

	8
	No lines, ladders or other rigging to be left outboard during transit, except for SPMs.
	

	8.1
	SPM1
	

	8.2
	SPM2
	

	8.3
	SPM3
	

	8.4
	SPM4
	

	9
	All machinery to be run-up and operating by
	

	10
	Bridge will be manned by:
	

	11
	Engine Room will be manned Expect xx hours manning
	

	12
	Coalition warships to be called on VHF Ch. 16 in case of emergency. – Ch 8 if Ch16 is being blocked or jammed
	

	13
	In case of an attack we will carry out a small zigzag manoeuvre, not more that xx - xx degrees rate of turn, else speed will drop and we may be more vulnerable
	

	14
	Four flares to be kept standby, to be used only on instructions from Master
	

	15
	In the event of vessel being pursued or suspected as being pursued raise the alarm, externally - Priority is VHF and DSC alerting
	

	16
	Music on channel 16 or jamming of Ch16 are to be viewed assigns of suspicious activity in the area.
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