S31 – CHECKLIST & PERMIT FOR ZEROING GUNS

	Test / Calibrate Aram and Ammunition
	

	Masters must ensure that:
	

	No member of the crew physically handles any of the arms placed onboard for the security of the vessel. 
	 FORMCHECKBOX 


	All testing / calibration, where practicable, must be done during daylight hours.
	 FORMCHECKBOX 


	A risk-assessed dedicated location on the poop deck, or other location, is to be identified for carrying out the testing / calibration of the arms. 
	 FORMCHECKBOX 


	An area is cordoned off with access points manned (crewmember or security team). This area will be a no-go area for the crew of the vessel. 
	 FORMCHECKBOX 


	A first aid kit is available on location.
	 FORMCHECKBOX 


	Two fire hoses are to be rigged and ready for immediate use. 
	 FORMCHECKBOX 


	The crew have been advised and all accounted for prior to the testing / calibration of the arms. 
	 FORMCHECKBOX 


	If possible, a security drill should be planned for immediately after the testing / calibration of the arms.
	 FORMCHECKBOX 


	No cargo operations (e.g. tank cleaning) are to be conducted at the same time.  
	 FORMCHECKBOX 


	On tankers or gas carries, tank pressures are to be well below vent valve lifting pressure. 
	 FORMCHECKBOX 
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