                                                                                  Supplement to S19 – free form

SECURITY PATROL ROUTES

Master / SSO to make security Patrol Routes specifically pertaining to their vessel, going by the below example.

	No.
	ROUTE DESCRIPTION
	SCHEDULE

	
	
	LEVEL 1
	LEVEL 2
	LEVEL 3

	1
	Anchor chain/hawse pipes/Spurling Points/ Chain Lockers -forecastle-fwd mooring ropes-fwd fire wire-main deck - waterside- quayside- aft fire wire-aft mooring ropes ER accesses- deck stores-CO2 room- emergency generator room- accom decks life boat-rescue boat- safety store -funnel area-bridge deck-monkey island deck
	Normal operations- Security rounds to be combined with safety rounds
	Security patrol every 1 hour (ACCESSES) using routes 1 / 2 alternating each even hour and routes  3 / 2  altern. each odd hour
	Constant (30 MINS) security patrol using routes1/2, 2/3  alternating each even hour and numbers 2/1, 1/3 altern. each odd hour

	2
	Lifeboat -rescue boat -safety store -accom decks-bridge deck-monkey island deck -funnel area emergency generator room -CO2 room -aft mooring ropes- -ER accesses- deck stores aft fire wire-main deck- waterside- quayside-fwd fire wire- fwd mooring ropes-anchor chain/hawse pipes-forecastle
	
	
	

	3
	Aft mooring wires- deck stores - CO2 room -ER accesses aft fire wire-life boat- rescue boat- safety store -accom decks- emergency generator room bridge deck - funnel area - monkey island deck- waterside- quayside-main deck-forecastle- fwd fire wire-fwd mooring ropes-anchor chain/hawse pipes 
	
	RESTRICTED AREAS MUST BE CHECKED AT LEAST TWICE PER WATCH
	RESTRICTED AREAS MUST BE CHECKED AT EACH PATROL

	Remarks:

1. SSO must periodically vary security patrol routes in order to avoid their determination by potential intruders

2. Security Patrol members have to check integrity of all restricted areas locks and plastic ties to ascertain if there has been unauthorised access.

3. Patrol should be equipped with torch, whistle and radio contact with OOW.

4. In case of level 3 security patrol must be double manned, if considered necessary.

	Patrols as per 6 hour watch in port

	5. 
	0100 hrs route 3
	route 2 + 1

	
	0200 hrs route 1
	route 1 + 2

	
	0300 hrs route 2
	route 1 + 3

	
	0400 hrs route 2
	route 2 + 3

	
	0500 hrs route 3
	route 2 + 1

	
	0600 hrs. route 1
	route 1 + 2


Note- Above is generic and can be adjusted by vessel to make ship specific
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