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CCR 14:  ANALYZERS - TOXIC GAS DETECTION TUBES CHECK
Each box of tubes must be recorded below.  Where there is more than one box with the same expiry date, each box is to be sequentially numbered. The tubes are to be checked at least every 3 months and the list maintained up to date.
	Date
	Tube type
	Range ppm
	Maker
	Date of expiry
	Signature and Rank

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


