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CCR 19:  REMOTE ULLAGING SYSTEM CHECK

A comparison should be made monthly between the remote ullaging system and the reference height in accordance with the Company instructions.
Where there is a difference of 1 cm or more, the remote ullaging system is to be corrected in accordance with the manufacturer’s instructions.
Overhaul and inspection of tank gauging equipment should be conducted every 6 months.
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