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CCR 20:  REMOTE TEMPERATURE MEASURING SYSTEM CHECK

Cargo tank fixed temperature measuring readouts must be compared against a UTI tape thermometer at least every 3 months.  The UTI tape must itself have been checked against a reference thermometer immediately beforehand.

If more than one readout per tank is fitted, the checks should preferably be carried out when the temperature throughout the tank is essentially uniform.

	Date
	Cargo tanks
	Condition
	Reference thermometer temperature
	UTI temperature
	Fixed system temperatures
	Signature and Rank

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	


