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CCR 21:  PRESSURE GAUGE TEST
Each pressure gauge is to be individually marked and checked against the reference pressure gauge at least every 12 months.  Where there is a difference of more than 10% the pressure gauge should be replaced. Each gauge must be protected by a valve or cock, which should be in good order.

	Date 
	Gauge no.
	Reference gauge pressure
	Pressure Gauge 
	Signature and Rank

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


