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CCR 25:  UTI TAPE CONDITION AND BONDING CHECK
UTI tapes are to be individually numbered.  The condition of the unit tape, detector should be checked in a metal container of water, including the external bonding wire and clip where fitted, is to be checked at least every 1 months according to the manufacturer’s maintenance instructions. Where the unit has internal bonding, this must be checked by a qualified person at least every 6 months. The temperature sensor must be compared against a reference thermometer at least every 3 months, and the date recorded on this form. UTI must be sent for shore service on annual basis.
	Date
	UTI tape no.
	Condition
	Bonding check
	UTI temperature
	Reference temperature
	Signature and Rank

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	


