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CCR 29:  CARGO SYSTEM PIPEWORK TEST
The discharge side of the cargo piping system should be pressure tested annually to 150% of the max working pressure using cargo pumps. The lines must be marked with the date of test and test pressure.  Positive displacement pumps should not be used for conducting cargo and crude oil wash line pressure tests.

Visual inspections, where practicable, must include the condition of pipework, the extent of rust, the condition of bolts and nuts, and the condition of couplings, where fitted.
	Date
	Cargo line
	Test pressure
	Visual inspection result
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