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CCR 31:  CARGO SYSTEM SEA VALVE CHECK
Prior to arrival at loading or discharge ports the sea valves should be pressurised to a maximum of 3.5 kg/cm2 (50 psi) and the pressure observed over a period of 15 minutes to ensure that it does not dissipate.  If it does then there is likely to be leakage.  Care should be taken that test pressures do not exceed 3.5.kg/cm2.
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