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CCR 33:  PORTABLE CARGO HOSE PRESSURE AND INTEGRITY CHECK
Portable cargo hoses must be marked in accordance with the requirements and should be visually inspected and pressure tested at least annually. Electrical bonding check of cargo hoses including emergency portable cargo pump hoses to be checked each operation.
	Date
	Cargo hose no.
	Examination result, condition, and remarks
	Continuity         <0.75 Ω / metre
	Test pressure
	Initial length
	Pressurised length
	Signature and Rank

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	



