	         CCR-34
	
	Form No.: CCR-34

	
	
	Revision: 01
Date: 15 Oct 2024

	
	Cargo Tank Ventilation Pipework
	Issued by: DPA

Approved by: MD

	
	
	Page: 1 of 4



CCR 34:  CARGO TANK VENTILATION PIPEWORK CHECK
Cargo tank ventilation pipework can normally only be visually inspected or checked for leakage during cargo operations.  Such checks should be carried out at least every six months. Cargo tank ventilation pipework to be pressure tested every 12 months.
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