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CCR 35:  CARGO TANK HEATING COIL TEST

Cargo tank heating coils should be hydrostatically pressure tested, up to a maximum of 7 kg/cm2, at least at 12 monthly intervals, and also before each use and after repairs have been carried out, and when changing from a dirty to a clean cargo.
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