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CCR 38:  TANK CLEANING HOSE CONDITION AND CONTINUITY TEST
Each tank cleaning hose must be individually identified.  The condition and continuity of each hose must be checked at least every 6 months, but at least monthly if they are in continuous use.

	Date
	Hose no.
	Condition
	Continuity         <6 Ω / m
	Remarks
	Signature and Rank

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


