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CCR 39:  P/V VALVE CLEANING AND OPERATION CHECK

Each P/V valve is to be dismantled, thoroughly cleaned and checked for correct operation at least once every 12 months.  It is critically important that the pressure valve is intact and undamaged in any way, and that flame screens are intact.
The Chief Officer should note that a more frequent cleaning routine might be required depending on the cargoes being carried.
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