	         CCR-40
	
	Form No.: CCR-40

	
	
	Revision: 01
Date: 15 Oct 2024

	
	PV Valve Flame Screens
	Issued by: DPA

Approved by: MD

	
	
	Page: 1 of 4



CCR 40: P/V VALVE FLAME SCREEN CHECK
Flame screens should be checked at least every 3 months and should be clean, free of corrosion, and completely intact.  Under no circumstances must a flame screen be re-used if there is any doubt about its integrity.

	Date
	P/V vacuum valve
	Result
	Signature and Rank

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	


