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CCR 44:  CARGO SYSTEM VAPOUR TEST – NON-IG
(Including vessels fitted with a Nitrogen Generator)

A leak test in accordance with the instruction Company Instructions and in accordance with requirements of USCG 40 C.F.R.§ 63.565 should be conducted at intervals not exceeding one year, whilst the tanks are being loaded and are at or above 80% full.
Vessel:
____________________
Operator:


IMO No.:
____________________



	Test Procedure

	A leak test in accordance with the instructions in Company Instructions, the cargo system (hatches, apertures, flanges, vapour locks, valve stems, drain cocks, valves) should be leak tested with a hydrocarbon analyzer at intervals not exceeding one year, whilst the tanks are being loaded and are at or above 80% full.  Should a leak be detected then it must be dealt with.  If the precise location of leak cannot be determined, then the use of soapy water should be considered.  The results are to be recorded in the table below.


	Cargo Compartment

	Port
	Date
	Loading Time

	Result 
	Name / Rank
	Signature

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	


All areas and equipment above cargo compartments, including hatches, apertures, flanges on vapour and cargo lines, vapour locks, valve stems, p/v valves, drain cocks and valves, and pumps have been tested in accordance with the procedure above and have been proved to be free of vapour leaks. 
Date of submission report:


_______________________
Name and Rank of person submitting report:
_______________________ 

Signature:




_______________________
