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CCR 46:  BALLAST TANK INERTING EQUIPMENT CHECK 

Each inerting hose, where fitted, should be marked with an individual identification number.  The following must be checked at 3 monthly intervals:

· The condition of each inerting hose, and the continuity;
· The condition of flanges and bolts on the inert gas main and, where applicable, the segregated ballast tanks;

· The condition of the 2 metre portable stand pipe and P/V Valve
	Date
	Hose no.
	Condition
	Continuity            <0.75 Ω per metre
	Remarks
	Signature and Rank

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


