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CCR 48:  BALLAST SYSTEM PIPEWORK TEST

Ballast pipework should be subject to a maximum of about 3,5 bars pressure in service and should be tested annually to about 150% in conjunction with ballast tank inspections.
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