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CCR 49: BALLAST VALVES CHECK
Ballast valves should be tested for tightness every 6 month.  This is achieved by ensuring that all ballast tank valves are closed, and by opening line and sea valves to pressurise the system. Ballast valves function test to be conducted monthly reference should be made to maker’s manual for open/close timing. 
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