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CCR 49(a): CARGO VALVES CHECK
Cargo valves should be tested for tightness every 6 month.  Cargo valve’s function test to be conducted monthly, reference should be made to maker’s manual for open/close timing.
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