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CCR 50:  CARGO VAPOUR HOSE CHECK
Vapour hoses should be visually checked for condition at least every 6 months.  If there is any doubt as to the integrity of a vapour hose it should be removed from service and pressure tested to at least 150% of its maximum rated pressure.
Each hose must be individually marked to allow for identification.

	Date 
	Vapour hose no.
	Test pressure
	Result
	Signature and Rank

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	



