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CCR 51: P/V Breaker Check
Flame screens should be checked at least every 3 months and should be clean, free of corrosion, and completely intact.  Under no circumstances must a flame screen be re-used if there is any doubt about its integrity. Glycol /Water liquid to be filled up as per maker instruction at Atmospheric Pressure.
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