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THIS CHECKLIST IS TO BE COMPLETED BY THE CHIEF OFFICER PRIOR TO USE

OF SHIP’S VAPOUR EMISSION CONTROL SYSTEM AND A DECK LOG BOOK ENTRY MADE
	HAVE THE FOLLOWING BEEN UNDERTAKEN:

	Initials

	Have the vapour return lines been visually inspected to ensure that they are clean and dry?
	

	Have manual valves been correctly positioned?
	

	Has vapour connection been properly made?
	

	Has an insulating device been fitted?
	

	Have the internal loading and maximum transfer rates been confirmed?
	

	Have the maximum and minimum operating pressures been confirmed?
	

	Have the alarms been tested within the previous 24 hours?
	

	Has the automatic shutdown system been tested within the previous 24 hours?
	

	Has oxygen plus other gas analysers been tested with span gas during the previous 24 hours?
	

	Is the condition of the vapour recovery hose satisfactory?
	

	Is the oxygen content in the vessels cargo tanks, if inerted, at or below 7%?
	

	Is the vessel unable to move under its own power within 30 minutes?
	

	Are flame screen fitted and maintained in good condition?
	

	Is there any authorized craft alongside?
	

	Are warning signals visible?
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