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THIS CHECKLIST IS TO BE COMPLETED BY THE OFFICER ON WATCH

AT LEAST ONCE PER WATCH AND A DECK LOG BOOK ENTRY MADE
	HAVE THE FOLLOWING BEEN UNDERTAKEN:
	Initials

	Is the vessel securely moored and is the deck watch maintained properly? 
	

	Have tidal ranges, tidal or river currents and vessel traffic movements which may affect mooring safety been continuously monitored for unpredicted changes?   
	

	Have weather forecasts been obtained at least once each watch from relevant sources, including NAVTEX, the information recorded and relevant changes and trends passed between watch keepers?
	

	Are fire wires rigged and maintained above water as agreed with terminal?
	

	Is the cargo loading and de-ballasting plan being adhered to?
	

	Is the vessel’s stress and stability within the acceptable limits?
	

	Are cargo surveyors  being accompanied by a ship’s officer?
	

	Are all unused manifolds, bends and spool pieces blanked?
	

	Is the radio and radar equipment isolated? (Including AIS if required by terminal)?
	

	Are offside manifold valves pressure gauges installed and the gauge “test” valve open? 
	

	Are all cargo manifolds not in use being monitored for pressure build up?
	

	Have cargo samples been taken?
	

	Has cargo heating, if required, been started?
	

	Are all sea valves closed, lashed and locked with suitable warnings posted? (lock out/tag out)?
	

	Are all deck scuppers plugged and is the deck clear of any oil or cargo leakages?
	

	Are all save alls clear, dry and plugged?
	

	Are ullages checked, and recorded with loading rates being calculated every hour and compared with shore figures?
	

	Have empty tanks been checked for leakages?
	

	Is the safety equipment rigged and is protective equipment ready for use?
	

	Has the inert gas upriser sump drain been checked and found clear and sump empty?
	

	Is pumproom hydrocarbon and/or toxic vapour (if applicable) monitoring being recorded hourly)?
	

	Is fixed gas monitoring equipment operational?
	

	Are cargo tank high level and overfill alarm systems operational?
	

	Is a deck watch being maintained properly?
	

	Are all cargo lines and valves properly set and cross-checked by a further member of staff?
	

	Is there a continuous supply of compressed air available on deck?
	

	Are the requirements and agreements made within the Ship Shore Safety Check List (SSSCL) being complied with, including repetitive checks?
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