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THIS CHECKLIST IS TO BE COMPLETED BY THE CHIEF OFFICER

PRIOR TO DEPARTURE AND A DECK LOG BOOK ENTRY MADE
	HAVE THE FOLLOWING BEEN UNDERTAKEN:
	Initials

	Have all manifolds, cargo lines, flexible hoses and loading arms been adequately blown/ drained /purged as necessary & pressure released prior disconnecting?
	

	Have all cargo and ballast system valves been closed and cross-checked by another member of crew?
	

	Are cargo surveyors being accompanied by a ship’s officer?
	

	Have all ullages, temperatures and samples been taken & sample retained onboard safely ?
	

	Are all manifolds, spool pieces and bends been blanked?
	

	Are all save-alls clear of cargo?
	

	Are all scupper clear of cargo?
	

	Have cargo calculations been completed, cargo documents agreed and, if required, appropriate protests been issued?
	

	Has the cargo tanks pre-washing operations, if applicable, been completed?
	

	Have all tank openings been closed?
	

	Is the vessel’s stress and stability within permitted limits for intended voyage?
	

	Is the vessel upright, properly trimmed and ready for sea?
	

	Have all shore connections including bonding cable been disconnected and are clear of the ship?
	

	Has the sea chest valves visually confirmed to be closed and lashed?
	

	Are all vapor locks closed?
	

	Are all the elbow connected to VECS system removed or valve locked as appropriate?
	

	Have all cargo hoses and deck gear securely lashed?
	

	Has all safety, firefighting and oil spill equipment been stored securely away?
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