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THIS CHECKLIST IS TO BE COMPLETED BY THE OFFICER ON WATCH AT LEAST 

ONCE PER WATCH AND A DECK LOG BOOK ENTRY MADE

	HAVE THE FOLLOWING BEEN UNDERTAKEN:
	Initials

	Is the vessel securely moored and is the deck watch maintained properly?
	

	Have tidal ranges, tidal or river currents and vessel traffic movements which may affect mooring safety been continuously monitored for unpredicted changes?    
	

	Have weather forecasts been obtained at least once each watch from relevant sources, including NAVTEX, the information recorded and relevant changes and trends passed between watch keepers?
	

	Are fire wires rigged and maintained above water as agreed with terminal?
	

	Is the cargo discharge and ballasting plan being adhered to?
	

	Is the vessel’s stress and stability within acceptable limits?
	

	Are cargo surveyors being accompanied by a ship’s officer?
	

	Are all unused manifolds, bends and spool pieces/connections blanked?
	

	Is the radio and radar equipment isolated? (including AIS if required)?
	

	Are all cargo manifolds not in use being monitored for pressure build up?
	

	Have cargo samples been taken?
	

	Is cargo heating, if required, being monitored?
	

	Are all sea valves closed, lashed and locked with suitable warnings posted?
	

	Is the sea valve pressure gauge still indicating a zero reading?
	

	Are all deck scupper plugged and is the deck clear of any oil or cargo leakages?
	

	Are all save-alls clean, dry and plugged?
	

	Are ullages checked, and recorded with discharge rates being calculated every hour and compared with shore figures?
	

	Have empty tanks been checked for leakages?
	

	Is the safety equipment rigged and is protective equipment ready for use?
	

	Is the pumproom and the cargo pumps being checked hourly?
	

	Is the pumproom hydrocarbon and/or toxic vapour (if applicable) monitoring being recorded hourly?
	

	Is the pumproom ventilation in operation and properly set up?
	

	Is the inert gas system, if in use, functioning correctly?
	

	Is the cargo tanks cow/pre-washing plan, if applicable, being adhered to?
	

	Are all cargo lines and valves properly set and cross-checked by a further member of staff?
	

	Is there a continuous supply of compressed air available on deck and have pneumatic spill pumps been tested?
	

	Are the requirements and agreements made within the Ship Shore Safety Check List (SSSCL) being complied with, including repetitive checks?
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