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	Vessel Name
	MV/ MT: 


	Date (yyyy-mm-dd)
	2025-01-01
	
	
	
	
	
	
	
	
	

	Drinking Water Tank/Tanks Last Date of Inspection, Cleaning and Disinfection with Chlorine
	

	Water Source – Ship / Shore
	Ship
	
	
	
	
	
	
	
	
	

	##Location from where sample is taken
	Galley
	
	
	
	
	
	
	
	
	

	
	Test Result

	*Residual Chlorine/ CLO
	0.3ppm
	
	
	
	
	
	
	
	
	

	#If applicable, details of the corrective action taken.
	NA
	
	
	
	
	
	
	
	
	

	*Total Content of Micro-organisms
	20
	
	
	
	
	
	
	
	
	

	#If applicable, details of the corrective action taken.
	NA
	
	
	
	
	
	
	
	
	

	Name of officer carrying out the Test
	
	
	
	
	
	
	
	
	
	

	Signature of officer carrying out the Test
	
	
	
	
	
	
	
	
	
	

	Name and Signature of Master
	
	
	
	
	
	
	
	
	
	


* Enter the reading as per the kit. # Refer to maker’s instructions for corrective action. Take Company approval before implementing corrective action. ## The Sampling points could be taken any of the following point: Water treatment processes, Water from drinking water tanks, Taps in the galley, and Points elsewhere on the pipelines, especially near the end of a pipeline. 

Remarks: 1. Residual Chlorine/ CLO:  The test kit gives the reading between 0.2 to 0.5 ppm. Color comparison is to be made in ten seconds. The result is to be decided within one minute as higher duration will give erratic readings. Detailed instructions are given in the maker instructions. 

2. Total Content of Micro-organisms – Refer to maker’s instruction manual. 

3. Red points i.e. Colonies of micro-organisms shall be generated on the culture paper. Number of red points is to be counted. If it exceeds one hundred, the water is to be disqualified and if it is less then hundred the water is good for drinking
Important - In case of Failure Test - Master should immediately inform the TSI along with the maker’s recommendation for the approval from the TSI. The additives as per maker’s recommendation shall be added only after the approval from Company / PIC.

Note: 1. Increase space as required 2. To be used every month 3. Retention period of this record on board in hard copy is 1 year (Liberian vessels: 3 years).

