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DAILY CHECKS

	Chk Box
	Sr No
	Description

	
	
	

	 FORMCHECKBOX 

	1 
	Check funnel smoke.

	 FORMCHECKBOX 

	2 
	Check for any leakage of Compressed air,  SW especially under bilge’s, etc. rectify all leakage.

	 FORMCHECKBOX 

	3 
	Take soundings of all dirty oil tanks. If filled up abnormally since last watch, take remedial action. Transfer sludge as required.

	 FORMCHECKBOX 

	4 
	Check for any abnormal operation or unusual noise from all running machinery.

	 FORMCHECKBOX 

	5 
	Blow through boiler Gauge, scavenge drains and soot blow the Exhaust boiler twice daily after informing bridge.

	 FORMCHECKBOX 

	6 
	Blow through Standby Generator and check operational readiness (specifically check running A/E rocker arm lubrication).

	 FORMCHECKBOX 

	7 
	Carry out water wash of Turbo charger blower side and solid wash of turbine side.

	 FORMCHECKBOX 

	8 
	Check and confirm emergency generator is always on “Auto-Standby”.

	 FORMCHECKBOX 

	9 
	Transfer F. O as per C/E’s instructions.

	 FORMCHECKBOX 

	10 
	Pumping out of Engine Room bilges to be carried in accordance with MARPOL Rules only.

	 FORMCHECKBOX 

	11 
	Check air to ship’s whistle is open at all times, drain pneumatic control system.

	 FORMCHECKBOX 

	12 
	Check drinking water tank level, change over consumption or filling, if required. Check hydrophore tanks & charge air if required.

	 FORMCHECKBOX 

	13 
	Check JCW, L.O, Cooler’s auto control valve position. Ensure normal working. 

	 FORMCHECKBOX 

	14 
	Check L.O storage tank levels.

	 FORMCHECKBOX 

	15 
	Check steering operation & equipment operations. Compare rudder movement with rudder angle indicator. Ensure all greasing satisfactory. 

	 FORMCHECKBOX 

	16 
	Inspect E/R for loose/improperly secured items, including tools, spares, L.O drums, steel plates, bars and pipes. Secure as necessary.

	 FORMCHECKBOX 

	17 
	Check Accommodation Blowers ensure heating / cooling as per requirement.

	 FORMCHECKBOX 

	18 
	Take a round in forward and aft hydraulic pump rooms and confirm every thing is normal. (Round to be taken by out-going watch-keeper).

	 FORMCHECKBOX 

	19 
	Identify any potential fire hazard. Take suitable action to eliminate same.

	 FORMCHECKBOX 

	20 
	Check Main Engine and AE L O sump levels are sufficient.

	
	21 
	Check flwg of ME: 1. Cylinder lubricator 2. All parameters  3. OMD

	 FORMCHECKBOX 

	22 
	Reduce bilge level to minimum.

	 FORMCHECKBOX 

	23 
	Cooling water tests and Boiler water tests to carry out and record. Cascade Tank Level and Temp. 

	 FORMCHECKBOX 

	24 
	Function test and lamp test of all control panels / alarm panels & MSB.

	 FORMCHECKBOX 

	25 
	Check insulation of 440 volt & 220/110 volt panel.

	 FORMCHECKBOX 

	26 
	Ensure all standby machinery in satisfactory condition.

	 FORMCHECKBOX 

	27 
	Back flush auto filters on F.O. and L.O. systems.

	 FORMCHECKBOX 

	28 
	Top up cylinder oil day tank.

	 FORMCHECKBOX 

	29 
	Check chemical dosing of Boiler and Fresh water generator.

	 FORMCHECKBOX 

	30 
	Confirm with bridge that fire alarms for all zones are active and not isolated.

	 FORMCHECKBOX 

	31 
	Check Log book is properly filled and updated.

	 FORMCHECKBOX 

	32 
	Acetylene and Oxygen bottles are secured and shut off immediately after use.

	 FORMCHECKBOX 

	33 
	E / Room crane parked and secured properly.

	 FORMCHECKBOX 

	34 
	Emergency escape checked for proper lighting and no obstructions.

	 FORMCHECKBOX 

	35 
	De-sludge all purifiers to confirm proper operation.

	 FORMCHECKBOX 

	36 
	Check FO System for any leaks. 

	 FORMCHECKBOX 

	37 
	ME JCW expansion tank. 

	 FORMCHECKBOX 

	38 
	Check Air Condition/ Refer system parameters.  

	 FORMCHECKBOX 

	39 
	Check Sewage plant operation/ SS p/P for leaks. 


WEEKLY CHECKS
	Chk Box
	Sr No
	Description

	
	
	

	 FORMCHECKBOX 

	1 
	Steering gear room bilge pumping out arrangement.

	 FORMCHECKBOX 

	2 
	SCBA Compressor for correct operation, filter and lubricating oil.

	 FORMCHECKBOX 

	3 
	Hold Bilge Alarms (where applicable).

	 FORMCHECKBOX 

	4 
	Emergency Batteries Checking: Including GMDSS batteries and Emergency generator batteries.

	 FORMCHECKBOX 

	5 
	CO2 Room Inspection: for correct bottle pressures and ventilation of the space.

	 FORMCHECKBOX 

	6 
	General Alarm and fire alarms. Alarm at every location to be tried out such that in a quarter all are tested.

	 FORMCHECKBOX 

	7 
	L/B Davit Safety: including limit switch and motor.

	 FORMCHECKBOX 

	8 
	EM. Generator & Starting Arrangements

	 FORMCHECKBOX 

	9 
	ECR Engineer’s Call Alarm

	 FORMCHECKBOX 

	10 
	Boiler Safeties

	 FORMCHECKBOX 

	11 
	Life Boat Engines tests as per the Maker’s Manual

	 FORMCHECKBOX 

	12 
	Emergency Fire Pump tests as per Maker’s Manual

	 FORMCHECKBOX 

	13 
	E/R Blower / Blower duct Flaps

	 FORMCHECKBOX 

	14 
	Funnel Flaps

	 FORMCHECKBOX 

	15 
	EM. Air Compressor

	 FORMCHECKBOX 

	16 
	Purifier, Emergency generator, hydraulic pump room Flaps

	 FORMCHECKBOX 

	17 
	Fire Hydrant, Hose & Nozzle

	 FORMCHECKBOX 

	18 
	Emergency lighting 

	 FORMCHECKBOX 

	19 
	Embarkation Lights

	 FORMCHECKBOX 

	20 
	Sand Boxes

	 FORMCHECKBOX 

	21 
	Fire Doors

	 FORMCHECKBOX 

	22 
	Cargo P/P trips

	 FORMCHECKBOX 

	23 
	Portable fire extinguishers

	 FORMCHECKBOX 

	24 
	

	 FORMCHECKBOX 

	25 
	

	 FORMCHECKBOX 

	26 
	

	 FORMCHECKBOX 

	27 
	

	 FORMCHECKBOX 

	28 
	

	 FORMCHECKBOX 

	29 
	

	 FORMCHECKBOX 

	30 
	

	 FORMCHECKBOX 

	31 
	

	 FORMCHECKBOX 

	32 
	

	 FORMCHECKBOX 

	33 
	

	 FORMCHECKBOX 

	34 
	

	
	
	

	
	
	


MONTHLY CHECKS

	Chk Box
	Sr No
	Description

	
	
	

	 FORMCHECKBOX 

	1 
	Standby and Other Pumps

	 FORMCHECKBOX 

	2 
	A/C Compressor & Stand by Fridge Compressor

	 FORMCHECKBOX 

	3 
	E/R Crane , Cargo hose handling crane, Provision/Bunker Crane Safeties

	 FORMCHECKBOX 

	4 
	Change Over of All Pumps

	 FORMCHECKBOX 

	5 
	Provision Room Alarm

	 FORMCHECKBOX 

	6 
	Gangway Safeties

	 FORMCHECKBOX 

	7 
	Aux. Engine Safeties incl. O/speed trip test

	 FORMCHECKBOX 

	8 
	Emergency Bilge Pump Stop from deck

	 FORMCHECKBOX 

	9 
	F. O. transfer pump  stop from deck

	 FORMCHECKBOX 

	10 
	Sewage Plant Isolating V/V’s

	 FORMCHECKBOX 

	11 
	Sludge Pump stop from deck

	 FORMCHECKBOX 

	12 
	Inert Gas Plant running test

	 FORMCHECKBOX 

	13 
	Gas detector calibration and function test

	 FORMCHECKBOX 

	14 
	Sea Suction & Overboard v/v Free & Grease

	 FORMCHECKBOX 

	15 
	Valve gearing for remote operation of v/v’s. 

	 FORMCHECKBOX 

	16 
	Hospital alarm

	 FORMCHECKBOX 

	17 
	Emergency Bilge Suction

	 FORMCHECKBOX 

	18 
	Quick Closing Valves

	 FORMCHECKBOX 

	19 
	ER dead man alarm 

	 FORMCHECKBOX 

	20 
	

	 FORMCHECKBOX 

	21 
	

	 FORMCHECKBOX 

	22 
	

	 FORMCHECKBOX 

	23 
	

	 FORMCHECKBOX 

	24 
	

	 FORMCHECKBOX 

	25 
	

	 FORMCHECKBOX 

	26 
	

	 FORMCHECKBOX 

	27 
	

	 FORMCHECKBOX 

	28 
	

	 FORMCHECKBOX 

	29 
	

	 FORMCHECKBOX 

	30 
	

	 FORMCHECKBOX 

	31 
	

	 FORMCHECKBOX 

	32 
	

	 FORMCHECKBOX 

	33 
	

	 FORMCHECKBOX 

	34 
	

	
	
	

	
	
	


Note: Non UMS vessels to comply with requirement while at sea and for every watch. UMS vessel to comply with the requirement of this check list at noon every day while at sea. Few rows are kept intentionally blank for the vessel to fill in ship specific checks. 

1 copy - to be kept on board the vessel
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