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	Vessel
	:
	
	Port
	:
	
	Date
	:
	

	Cargo System

	
	Cargo Oil Pumps
	# 1 Ball
P/P
	# 2 Ball
P/P
	COW
P/P

	Manual Trips*
	1
	2
	3
	4
	
	
	

	CCR
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	ECR
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Pumproom Top
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Pumproom Bottom
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Port Manifold
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Starboard Manifold
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Turbine Side
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Pump Auto Protection Devices
	
	
	
	
	
	
	

	Casing High Temp
	(Set Point oC)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Upper Bearing High Temp
	(Set Point oC)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Lower Bearing High Temp
	(Set Point oC)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Casing High Press
	(Set Point kg/cm2)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Turbine Auto Protection Devices
	
	
	
	
	
	
	

	Overspeed {Electrical}
	(Value rpm)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Overspeed {Mechanical}
	(Value rpm)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Lub Oil Low Press
	(Set Point kg/cm2)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	High Exhaust Press
	(Set Point kg/cm2)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Turbine Upper Bearing HT
	(Set Point oC)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Turbine Lower Bearing HT
	(Set Point oC)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Turbine Thrust Bearing HT
	(Set Point oC)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Cargo Lines *
	Tested to:
	
	kg/cm2
	& all satisfactory
	 FORMCHECKBOX 


	Pressure Test Lines
	COW Lines
	Tested to:
	
	kg/cm2
	& all satisfactory
	 FORMCHECKBOX 


	
	MARPOL Line
	Tested to:
	
	kg/cm2
	& all satisfactory
	 FORMCHECKBOX 


	Miscellaneous
	

	COP & Ballast pumps ready for use*
	
	 FORMCHECKBOX 

	
	

	Integrity of COP and ballast pump mechanical seals confirmed**
	
	 FORMCHECKBOX 

	
	

	Stripping Pump tested and found satisfactory
	
	 FORMCHECKBOX 

	
	

	Pumproom bilge alarm tested and found satisfactory
	
	 FORMCHECKBOX 

	
	

	Pumproom bilges clean and dry
	
	 FORMCHECKBOX 

	
	

	Pumproom sea valve test procedure carried out satisfactorily

IG System Deck Non Return Valve free movement confirmed  
	
	 FORMCHECKBOX 

 FORMCHECKBOX 

	
	

	Clean instrumentation air filter.
	
	 FORMCHECKBOX 

	
	

	Instrumentation Air drained at all check points, and confirmed to be free of water and oil residues. 
	
	 FORMCHECKBOX 

	
	


* All COP's are to run up during the pre-arrival testing process thus integrity of main lines, risers etc and the applicable pump trips can be proven. However, in the case of the annual line pressure testing the use of the stripping pump will be required.  It should be ensured that bottom lines are not subjected to any pressure testing during this process.
** In addition, previous operations should be used as a guidance for any possible overhaul / maintenance of the applicable seals.

	Vessel: 
	Port: 
	Date: 

	Inert Gas System

	
	Recorded Value
	Alarm
	Trip

	Deck Seal
	Seal Water Supply
	Low Flow
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Seal Water Supply
	Low Press
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Deck Seal
	Low Level
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Scrubber
	Cooling Water
	Low Flow
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Cooling Water
	Low Press
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Venturi or pre-cool
	Low Flow
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Venturi or pre-cool
	Low Press
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Sealing Water
	Low Flow
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Sealing Water
	Low Press
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Seal Chamber
	Low Level
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Scrubber Tower
	High Level
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Fix Oxygen Analyser 
	Sensor 

Sensor  
	High 

Low
	



	 FORMCHECKBOX 

 FORMCHECKBOX 

	 FORMCHECKBOX 

 FORMCHECKBOX 


	Others
	Deck Main Pressure
	High
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Deck Main Pressure
	Low
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Deck Main Pressure
	Low Low
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Oxygen
	High
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Control Air Pressure
	Low
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Control Panel Elect Source
	Fail
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Alarm Value
	Alarm
	Trip Value
	Trip

	
	
	1
	2
	3
	
	1
	2
	3

	Fans ***
	Fan discharge high pressure
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Fan discharge high temp
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Electric motor fail
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Inert Gas Burner
Recorded Status
Yes
No
IGG Burner
Burner Cleaned
Condition
 FORMCHECKBOX 

 FORMCHECKBOX 

Flame
Condition
 FORMCHECKBOX 

 FORMCHECKBOX 

Fuel Leakage
Oil Press
 FORMCHECKBOX 

 FORMCHECKBOX 

Exhaust
Funnel Smoke
 FORMCHECKBOX 

 FORMCHECKBOX 



	

	Confirmation Checks

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	Miscellaneous

	
	
	
	
	

	
	
	
	
	

	Signature:                                                                        

	
	Date
	Time
	Signature

	Duty Engineer
	
	
	

	2nd Engineer
	
	
	

	Chief Engineer
	
	
	


*** As far as is practicable and considering the number of starts allowed, the IG fans should be run up thus applicable trips are positively confirmed.  This will also prove the correct operation of all applicable control valves on the IG system

