	[bookmark: _Hlk186123503]HSSEQ-07A
	
	Form No.: HSSEQ-07A

	
	
	Revision: 01
Date: 15 Oct 2024

	
	Hot Work Concurrence (For Tanker Fleet)
	Issued by: DPA
Approved by: MD

	
	
	Page: 1 of 4

















	HSSEQ-07A
	
	Form No.: HSSEQ-07A

	
	
	Revision: 01
Date: 15 Oct 2024

	
	Hot Work Concurrence (For Tanker Fleet)
	Issued by: DPA
Approved by: MD

	
	
	Page: 1 of 4




	Vessel: 
	
	Date:
	

	Vessel Condition:
	Loaded*
	|_|
	Cargo Details
	
	Inerted vessel
	|_|

	
	Ballast
	|_|
	
	
	Non-inerted vessel
	|_|

	Details of the planned hot work:
	

	Other Details:
	Tank status within 30 metres radius 
	

	
	Status of Slop tanks
	

	
	Status / Distance of Bunker tank
	

	Area:
	Engine room (outside workshop)
Inside Accommodation
	|_|

[bookmark: check1]|_|
	
Aft open deck
Forward open deck
Over the side and ship’s hull            
	|_|
|_|
|_|
	Enclosed space
	|_|

	
	On pipelines
	|_|
	On or near tank deck
	[bookmark: check2]|_|
	In tank
In pump-room
	|_|
|_|

	Action Checklist 
(Documentation to the submitted to office for verification of below actions)
	Status

	A
	Work scope and requirement discussed & documented. 
	|_|

	B
	Radius of area to be cleaned for Hot work reviewed and confirmed. 
(Drawing / GA to be submitted to the office along-with the HWC request) 
	|_|

	C
	A written plan for undertaking the work to be completed, discussed and agreed by all who have the responsibility in connection with the work.
	|_|

	D
	Risk assessment, daily safety meeting and onsite toolbox meeting carried out.  
	|_|



	Work scope
	:
	

	Exact location
	:
	

	Reason necessary
	:
	

	Job Planned to be commenced 
(to be completed by Master)
	Date:
	
	Time:
	

	Expected job duration 
(to be completed by Master):
	



	A / Work scope and requirement
                                                                                      ITEMS HIGHLIGHTED IN GREY HAS TO BE COMPLETED AS MINIMUM

	Work location
Minimum Requirement
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	
	Other parts of non-hazardous area (e.g. Inside accommodation block) 
ER (Outside workshop)
	Open deck aft of accommodation
	Enclosed space other than PR
	Main deck plating        
	Work on fixtures/fitting on main deck
	Work on any cargo related pipelines incl. heating coils in a cargo tank
	Cargo Pump-room
	Cargo or Ballast tank 
	Over the side and ship’s hull            

	Work planning meeting completed – Document same under ‘C’ 
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Work Permit, Isolation and tagging requirements, and correct procedures discussed 
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Adequate ventilation carried out
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Confirmation from Master or Responsible Person that work is OK to proceed
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Tank atmosphere checks to be carried out and entry permit issued. (For hot work in cargo tank area (Tanker vessels) continuous monitoring of the atmosphere in the vicinity must be carried out during the entire duration of hot work. )
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Tank to be washed and gas free. Record the values in the Hot work permit HSSEQ-07. 
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Adjacent Cargo tanks within 30 meters radius to be purged and inerted to not more than 8% O2 and not more than 2% HC. 
For non-inerted vessels cleaned and gas free to HW standards or completely filled with water 
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Tanks opening closed 
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Inert Gas pressure reduced to prevent uncontrolled venting.
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Work to be carried out further than 500 mm from the tank deck or bulkhead or else classed as Hot work in tank. 
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Work to be carried out more than 500 mm from a fuel oil tank deck or bulkhead and clearly identified in the relevant drawing / plan 
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Relevant drawing / plan to identify the Work area, discussed in the Work plan meeting and send to office along-with this HWC. 
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Local cleaning to be carried out as per requirement.  
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	All interconnecting pipelines flushed and drained. Disconnected and remaining pipe work blanked off. 
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Tank valves isolated
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Welding and Gas equipment inspected and free from defects. Welding equipment adequately earthed. Welding cable routed through gas free or inerted space. . 
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Hot Work permit to be issued on board as per company procedures
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|

	Hot Work permit approved by Master
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|
	|_|



	[bookmark: _Hlk35355985]B / Radius of area to be cleaned for Hot Work

	Height of work
	OPERATOR SIDE
	OPPOSITE SIDE

	
	Gas cut
	Welding
	Gouging
	Gas cut
	Welding
	Gouging

	0-5 meters 
	1.5 |_|
	5.0 |_|
	4.0 |_|
	7.5 |_|
	2.0 |_|
	2.0 |_|

	5-10 meters 
	1.5 |_|
	5.0 |_|
	5.0 |_|
	10.0 |_|
	2.0 |_|
	2.0 |_|

	10-15 meters 
	1.5 |_|
	5.0 |_|
	7.5 |_|
	15.0 |_|
	2.0 |_|
	2.0  |_|

	>15 meters 
	1.5 |_|
	5.0 |_|
	10.0 |_|
	20.0 |_|
	2.0  |_|
	2.0 |_|

	C / A written plan for undertaking the work to be completed, discussed and agreed by all who have the responsibility in connection with the work: 
Planned Safety Precautions: (Including Tank Preparation): 



Master comments:



	D / Additional concerns if any:


Master comments: 



	Responsible officer (not connected to the Hot work designated to ensure the plan is followed) 

	[bookmark: _Hlk35527742]Responsible Officer Name (Chief Officer/ 2E/ CE) *:
*Delete as appropriate
	
	Signature:
	

	Master's name:
	
	Signature:
	

	For Office Use (only):

	Comments from Technical Superintendent  




	Name of TSI:
	

	Signature:
	

	Comments from Marine Superintendent




	Concurrence granted by Marine Superintendent:
	Yes |_| 
	[bookmark: Check3]No |_|
	Date:
	

	
	
	
	Time:
	

	Reason if denied:
	

	Name of MSI (Tankers): 
	
	Signature:
	



	Instructions:
[bookmark: _Hlk34747482]1. This form is to be completed for any hot work to be conducted on a vessel outside the engine workshop and sent to Office for evaluation and approval.
2. No hot work is permitted outside the engine room or accommodation block during loaded passage, unless considered essential for the safety of the crew or the immediate operational capability of the ship. 



	Master’s Name: 
Signature:                          Date and Time of Completion of Hot work:

























