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	Vessel
	:
	
	Date
	:
	

	All joining or rejoining crew are required to have the following minimum training and familiarization onboard with regards to lifting appliances.
Section A - Needs to be completed prior to first use of the lifting appliances by a crew member 
Masters may arrange for further familiarization and training that may be necessary for the vessel.  

On completion of each training section, the joining crew, the on site instructor, and the Chief Officer or Chief Engineer shall sign and date the section completed.

Section B - This checklist need to be completed each time the lifting appliance is being used. 

Publications to be consulted: RECOMMENDATIONS FOR THE TAGGING/LABELLING, TESTING AND MAINTAINENCE, DOCUMENTATION/ CERTIFICATION FOR SHIPS’ LIFTING EQUIPMENT
Ships Cargo gear consist of following equipments: 

· Cargo Horse crane / derrick

· Provision Crane 

· E/R Cranes 

· Any other lifting appliances as considered by the Ship staff as a lifting appliance  

NOTE: RECTIFY THE CONDITION BEFORE OPERATION, IF ANY OF BELOW CHECKS LISTED ARE NEGATIVE.


	
	Item
	Yes
	No

	
	SECTION A: Familiarization
	
	

	
	Conduct familiarization and training to operate the equipment. Within 30 days of joining or prior First time use (which ever is earlier). 
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Have items listed under Sec 2 been demonstrated to the Officer / Crew to ensure they have fully understood the working of the equipment 
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Limit switches and brakes are operational. 
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Emergency stop is operational.
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Ensure that all crane operations (hoisting, luffing and slewing) are satisfactory
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	All sheaves & other moving parts are freely moving without any abnormal noise.
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	If the equipment has Hydraulic machinery ensure following:

	
	Operate hydraulic power packs as per instructions posted on the starting panel.
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Ensure oil level of service tank is within operating limits.
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Ensure oil-cooling mechanism is in operation.
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Ensure there are no leaks in any hydraulic pipes / hoses and fittings..
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	In cold weather conditions operate with load only when the hydraulic oil temp rises above a minimum value specified by manufacturers
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	If the equipment has Electric / Travelling Gantry machinery ensure following:

	
	Check the push buttons are activated properly in the direction indicated on the remote-operating panel.
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Check if voltmeter indicates the specified voltage in allowable range.
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Check through the travelling rail including the stoppers for any obstruction.
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	
	Ensure that the travelling and transverse clamp gears are not clamped.
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	SIGNATURE
	SIGNATURE 

	Name of Officer / Crew Undergoing Familiarizations 
	
	Name of Officer  conducting Familiarizations 
	

	Date: 
	
	Date: 
	


	
	Item
	Yes
	No

	
	SECTION B – CHECKLIST TO BE USED PRIOR EACH USE
	
	

	A.
	Is cargo gear register up to date with all required entries?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	B.
	Has annual examination been completed in last 12 months?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	C.
	Has yearly examination / testing been done?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	D.
	Are test certificates available for all lifting equipment (max 5 years)?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	E.
	Is the rigging plan available and is it correct?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	F.
	Is identifying marks stamped in lifting gear and is it legible?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	G.
	Do these marks tally with cargo gear register?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	H.
	Are all wires in good condition with no broken strands?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	I.
	Are sheaves free, well greased and in good condition with no grooves?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	J.
	Are all swivels working and well greased?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	K.
	Are cranes marked with SWL?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	L.
	Are crane angle indicators working?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	M.
	Are limit switches adjusted properly and working?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	N.
	Are controls clearly marked and operating correctly?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	O.
	Do controls have locking devices to prevent accidental movement?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	P.
	Are brakes working and properly adjusted?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Q.
	Does crane “creep” under load?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	R.
	Is access to Operating area safe? (ladders in good condition with cage if applicable)
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	S.
	Have emergency stops in cabin been tested?
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	T.
	Has a Risk Assessment been conducted and discussed during the daily work plan meeting? 
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	U.
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	V.
	
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Filing
	
	1 Hard Copy onboard

	SIGNATURE
	SIGNATURE 

	Name of Officer / Crew using the equipment 
	
	Name of Responsible office 
	

	Date: 
	
	Date: 
	



