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	Vessel Name:
	Location where camera used:  

	Description of work:
	Personnel using the camera:

	This permit is valid from
	:
	
	Hrs LT
	Date:

	(Maximum validity 8 hours) to
	:
	
	Hrs LT
	Date:

	
	
	
	
	

	This Permit shall be complied with, whenever a non-intrinsically safe camera is required to be used in hazardous areas on board vessels. These areas are on the exposed decks outside accommodation spaces, outside engine room and within cargo / bunker / ballast tanks, pump room and void spaces.

	Description
	Yes
	NA
	Description
	Yes
	NA

	Risk assessment, daily safety meeting and onsite toolbox meeting carried out. 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	No cargo, bunkering, tank cleaning operations and venting of gases in progress
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	All cargo tanks inerted with O2 less than 8% OR gas free (if camera used on deck)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Combustible gas indicator reading is not more than 1% LEL at the location of work
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	If inerted, Cargo tank IG Pressure kept at minimum (not more than 500mmwg)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Port/Terminal permission obtained (if within port limits)
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Ballast tanks / void spaces are free of HC gases
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	There is no alternate safer method to complete the task  
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	“Personal Gas Monitor” carried 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Battery changed only inside accommodation 
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Mobile phones or other devices with camera not used
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Only one camera permitted at a time 
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Office informed where applicable
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	
	

	Additional points to be complied for use of camera in Cargo / Bunker / Ballast tanks

	Cargo / bunker / ballast tanks where the camera used are ventilated thoroughly
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	O2 content in the tank is 21% and LEL not more than 1%
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Enclosed space permit issued 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	
	
	


	Any special conditions/precautions:


	The above mentioned points have been checked and the conditions at the site, or of the equipment to be worked on, are safe for the work to be undertaken

	Rank
	Signature
	Date / time
	Rank
	Signature
	Date / time

	Responsible officer
	
	
	Master
	
	

	Person using camera
	
	
	
	
	

	PERMIT TO WORK CANCELLED (If prior to job completion, give reasons):


	Completion of job (To be completed by the responsible person) 

The work has been completed and all persons under my supervision, materials and equipment have been withdrawn. Camera power turned off. All persons involved advised and permit has ended

	Rank
	Name
	Date / time
	Signature

	Responsible officer
	
	
	

	Note: This permit is rendered invalid if any of the conditions noted in the checklist change


	CONTROLLED
	Revision: 15 April 2022

	
	Approved by DPA/DMR
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