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	Name of Vessel
	          

	Port of arrival and ETA
	                              /                       

	Date of completion of checks (A)
	          

	Previous date of completion of checks (B)
	          

	Confirm duration between A and B does not exceed 7 days for vessels engaged on coastal / short voyages.
	YES / NO*  
(*Delete as appropriate. Remarks are needed in-case of “NO”) 

	Is the vessel having any flag state acknowledgement, dispensation, short term certification or Condition of class due to any reason? (e.g., statutory, Technical, manning etc)
	Yes / No*   
(*Delete as appropriate. Remarks are needed in-case of “YES”)

	Has the port authorities been informed about the flag state acknowledgement, dispensation, short term certificate or condition of class as above?  
	Yes /N.A*  (*Delete as appropriate)
Date of notification to port: _____________
(DD-MMM-YYYY)

	Name of Master and Signature
	                              /                       

	Name of Chief Eng. and Signature
	                              /                       

	
Remarks / Non-compliance observed and office notification etc





	


Instructions on use of PSC readiness verification checklist
1. This checklist shall be completed by Master and C/E prior arrival every port.
2. For vessels calling ports more frequently and engaged on short voyages, if the checklist has been completed within the last 7 days it need not be repeated. (Max interval 7 days)
3. If vessel is shifting berths within same port, then checks prior arrival 1st berth would suffice subject to total port stay including anchorages does not exceed 7 days.
4. Section A of the checklist requires physical verification by master and C/E
5. Section B of the checklist requires data from other sources including assistance from other Officers as deemed necessary. However, the Master shall personally check the status of any item if in any doubt. 
6. If any deficiency is noted, it shall be immediately reported to TSI / TD over the phone , followed by in email  with CC to DPA & SNQ.
7. All deficiencies shall be recorded in Technical Defect List (TDL) for proper follow up.
8. Make entry in deck logbook for compliance to INSP-02 prior arrival. 
9. Technical Superintendent / Technical Director shall ensure compliance to FOM 1.1 section 6.0 on reporting the defects to flag state / class asper statutory obligations and guide master to notify to port authorities, PSC prior arrival. Flag state dispensation or acknowledgement must be obtained prior arrival.

	[bookmark: _Hlk528333436]Section A – Mandatory physical verification by Master and C/E

	Sn
	Item to be verified 
	Yes
	No
	N/A

	1
	Lifeboats  
· Engine operational running test ahead and astern on each battery separately. Check compliance to cold weather starting procedures if any.
· Steering test – Rudder has good freedom of movement hard to port and hard to starboard
· On-load release gear (if fitted) - Check and ensure mechanism is properly reset as per manufacturer’s instructions.
· C/E to verify fuel quantity for LB engine is as per operational booklet or class test report to meet SOLAS requirement.
	[bookmark: Check1]|_|
	[bookmark: Check2]|_|
	[bookmark: Check5]|_|

	2
	Rescue boat (If fitted) 
· Engine operational running test ahead and astern as per maker’s instructions.
· Steering test – Check as per maker’s manual and design
· C/E to verify fuel quantity for RB engine is as per operational booklet or class test report to meet SOLAS requirement.
· All crew familiar with launching method using primary and secondary means.
	|_|
	|_|
	|_|

	3
	Life rafts are properly secured on cradle and painter is connected to the weak link as per maker’s guidance.
	|_|
	|_|
	|_|

	4
	Emergency generator operational test in all available starting modes. 
	|_|
	|_|
	|_|

	5
	Fire Dampers – (use light test)
· Funnel flaps working satisfactory and able to achieve full sealing. 
· Engine room vent fans fire dampers remote activation and local shut off tested 
	|_|
	|_|
	|_|

	6
	Oily water separator (OWS) to be tested as below:
· OWS pump and flow meter functional test in recirculation mode with Overboard valve SHUT.
· 15 ppm alarm test, Oil Probe and 3-way valve changeover / Pump stop (as per design)
· Test shall be recorded in ORB part I under code I.
Note: Pre-arrival test can be combined with OWS monthly test as stated in SMS.
	|_|
	|_|
	|_|

	7
	Engine room bilge high level alarm system operational.
	|_|
	|_|
	|_|

	8
	Quick closing fuel valves: Check no temporary blocks to force valves in the open position and that all pneumatic lines are connected.
	|_|
	|_|
	|_|

	9
	Steering gear / purifier room fire doors must be SHUT. 
No holding back arrangements such as ropes, hooks and chains, etc.
	|_|
	|_|
	|_|

	10
	Overall housekeeping in engine room is satisfactory. No fuel oil, lube oil or hydraulic leaks on operating machinery and no oil-soaked lagging or rags. 
	|_|
	|_|
	|_|

	11
	Emergency fire pump working satisfactory, including priming pump if fitted. Pressure gauge indication on fire main to be verified.
	|_|
	|_|
	|_|

	12
	The fire detection system panel is fully operational and no errors / loop fault etc
	|_|
	|_|
	|_|

	
	Additionally for Tanker Vessels - 
	

	1
	Pump room fixed gas detection system is fully operational. No errors or faults.
	|_|
	|_|
	|_|

	2
	Overboard Discharge Monitoring Equipment (ODME) is fully operational. Print out must be legible.
	|_|
	|_|
	|_|

	3
	Pump room fire dampers closure satisfactory (Use light test)
	|_|
	|_|
	|_|



	Section B – Verification based on documents / assistance from officers

	Sn
	Item to be verified 
	Date of last check / test
	Master’s Initials

	1
	Seafarer Employment Agreement (S.E.A), flag state endorsements (COE/CRA) must be valid as per hard copies in file.
Weekly export of data to crewing PIC?
Note: All crew members must have a valid mutually agreed signed contract. Flag state communication to be onboard for any extended contracts / SEA for any crew member more than 10 months on board. Please specify details in remarks section on Page 1 if vessel has crew who have been onboard in excess of 10 months.
	
	

	2
	Statutory certificates available and valid 
	
	

	3
	Verify compliance to shipboard drill matrix. Drill records and relevant entries in Official log, Deck log-book and engine log book must be checked prior arrival port.
Flag state dispensation should be in place for overdue launching of lifeboat, rescue boat in water as per SOLAS requirement.
	
	

	4
	Verify Oil record book Part I /II and Garbage book Part I / II as applicable for proper entries.
Master’s signatures on completed pages of ORB/GRB
	
	

	5
	ECDIS / Paper charts are up to date to latest weekly NTM / NAVAREA / NAVTEX
	
	

	6
	Status of navigational lights, any alarms, and check condition of signalling appliances.
	
	

	7
	Master’s verification of periodic maintenance of life saving appliances and records of expiry dates (SSTRB). Confirm no LSA items are expired or due for expiry in next 7 days.
	
	

	8
	Master’s verification of periodic maintenance of firefighting appliances and records of expiry dates SSTRB/ HSSEQ-40 Confirm no FFA items are expired or due for expiry in next 7 days.
	
	

	9
	Master has conducted sample checks on work rest hours records and verified that records match actual operation of vessel. Samples should be spread to check officers, engineers, ratings for occasions such as drills, UMS, bunkering, pilotage.
	
	

	10
	Masters’ weekly accommodation inspection for MLC compliance.
Quality & quantity of victualling provisions and fresh water is verified, and records of checks maintained in deck log / Official log- book. 
	
	

	11
	MARPOL compliance checks: Environment seals  and .  Overboard discharge fro Sewage and Grey water to confirmed as locked with local Port guidelines requires nothing overboard. Verify that OWS test as required and  was conducted within last 30 days and recorded in ORB Part 1.

	
	

	12
	Records as per Technical Defect List (TDL), Structural inspection of critical hull parts such as piping system, soft patches and temporary MOC for it.
Ensure air vents on deck are thoroughly checked within last 3 months and condition is satisfactory. Any defect for air vents in TDL is properly followed up for urgent rectification.

	
	





















