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	Voyage No:
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	Readings
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[Note: 1: To be performed during each loading and discharge operation.]
[Note 2: Any large discrepancies on level readings must be reported to Company. acceptable ± 7.5 mm]
[Note3: Compare readings of local and remote level gauges on cargo system with the reference value at stowed position and the reference value at ball valve position]
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