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	Vessel:
	
	Voyage No.:
	

	Master:
	
	Port/Area:
	


	Item
	Description
	Ch.Off

Initials
	Cargo Eng

Initials

	1. 
	Megger test of cargo/spray pumps
	
	

	2. 
	Bolts and nuts secured
	
	

	3. 
	Pump spinning direction test
	
	

	4. 
	Cable securing
	
	

	5. 
	Bellows
	
	

	6. 
	Pipe supporters
	
	

	7. 
	Temperature sensors
	
	

	8. 
	High level shutdown system
	
	

	9. 
	Whessoe
	
	

	10. 
	Tower clearance
	
	

	11. 
	Spray nozzles
	
	

	12. 
	Vacuum clean, collect the dust
	
	

	13. 
	Number of tools brought into the tank
	
	

	14. 
	Number of tools brought out of the tank
	
	

	15. 
	Cargo and spray pumps shall be megger tested before commence inerting
	
	

	16. 
	Only safety approved lights to be used inside the cargo tank
	
	

	17. 
	Ch.Off and Cargo Eng are the last persons to leave the tank after proper inspection is made
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