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Port: 
	
	Yes
	No

	One hour before ESP, warm up and start alternators (for bow thrusters 3 Alternators should be in bus bar).
	
	

	Check if Diesel engine is in stand by-mode
	
	

	If possible, start a boiler soot blowing sequence to economizer (short program)
	
	

	Verify that all bilge / sewage overboard valves are secured with padlock
	
	

	Lock all access doors to engine room
	
	

	Close oxygen and acetylene bottles and vent the line
	
	

	Stop freshwater generators
	
	

	Shift sea suction from low to high
	
	

	Shift MGPS valves
	
	

	Take all relevant counters at official 'ESP'-time
	
	

	Test engine astern before arrival at pilot station (signal from bridge)
	
	

	During manoeuvring, the engineer on duty has to check regularly the engine room
	
	

	Manoeuvring finished : sub-telegraph to F.W.E. mode.
	
	

	Take all relevant counters at official 'FWE'-time
	
	

	After FWE, reduce electrical power (Bow thrusters, steering gear motor…) with the permission of bridge
	
	

	
	
	

	Shift control position from wheelhouse to ECR.
	
	

	With permission of bridge, engage the main turbine turning gear.
	
	

	Switch off cathodic protection system (fwd & aft)
	
	


	
	ESP
	On Anchor
	Drift on
	Anchor up
	Drift finish
	FWE

	Time
	
	
	
	
	
	

	M. Turbine rev counter
	
	
	
	
	
	

	Boiler fuel counter
	
	
	
	
	
	

	DG fuel counter
	
	
	
	
	
	

	Rob      HFO
	
	
	
	
	
	

	            MDO
	
	
	
	
	
	

	            LDO
	
	
	
	
	
	

	Flash FWG counter
	
	
	
	
	
	

	Sub. FWG counter
	
	
	
	
	
	


Engineer on duty





Chief Engineer
