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	  Yes
	No

	When departure is confirmed, advise Chief engineer and second engineer
	
	

	One hour before departure, ask permission from duty officer/captain to disengage turning gear for main  turbine warming up (auto spinning)
	
	

	
	
	

	Check if Diesel Generator is in st-by mode
	
	

	If not in service, warm up and start TA (3 Generators should be in bus bar for bow thrusters)
	
	

	Check alarm panels of main turbine, reset all alarms
	
	

	15 minutes before stand by, call bridge and wait confirmation for testing telegraph;      
A short time dead-slow astern on "ECR", and a short time dead-slow ahead on "wheelhouse control" and after that, keep main turbine control on "bridge control" position.
	
	

	Take all relevant counters at official 'St by'-time
	
	

	Take all relevant counters at official 'SSP''-time
	
	

	After SSP, reduce electrical power consumption (fire pump, bow thrusters) with the permission of the bridge, and stop unnecessary turbo alternators
	
	

	
	
	

	Shift sea suction from high to low
	
	

	Shift MGPS valves
	
	

	Start evaporators
	
	

	Operate all soot blowers 
	
	

	Switch on cathodic protection system (fwd & aft)
	
	

	After SSP, the engineer on duty has to make a serious round in engine room (check list) especially during night time
	
	



Date:								Port: 




Engineer on duty						Chief Engineer
	 
	SBE
	At anchor
	Anchor up
	SSP
	ISP
	RSP

	Time
	 
	 
	 
	 
	 
	 

	M/T rev. counter
	 
	 
	 
	 
	 
	 

	Boiler fuel counter 
	 
	 
	 
	 
	 
	 

	DG DO counter
	 
	 
	 
	 
	 
	 

	ROB :   HFO
	 
	 
	 
	 
	 
	 

	            MDO
	 
	 
	 
	 
	 
	 

	            LDO
	 
	 
	 
	 
	 
	 

	Flash FWG counter
	 
	 
	 
	 
	 
	 

	Sub. FWG counter
	 
	 
	 
	 
	 
	 
















