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	Vessel
	
	
	Port/Geographical area
	

	The vessel position to be recorded at least every 60 minutes. The interval can be reduced as per Master’s discretion e.g. in case of deteriorating weather conditions, traffic, available sea room.


	Date
	Time
	Vessel position
	Object 1 
(________)
	Object 2 
( ________)
	Distance from nearest vessel
	UKC
	Chart Depth
	Ship's heading
	Position fixing method

(Visual / GPS / Radar)
	Position of vessel with respect to Swinging circle (In/Out)
	Remarks
	Signature of OOW

	
	
	Lat
	Long
	Bearing
	Distance
	Bearing
	Distance
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