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	Ship’s Name
	
	Barge Name
	

	Own’s Ship’s Freeboard
	
	Barge Freeboard
	

	Own Ship’s LOA
	
	Barge LOA
	

	Date 
	
	Transfer Location
	

	Master reserves the right to abort the transfer operation if:

· The fendering, permissions or equipment to conduct a safe transfer is adequate.

· The weather, sea or swell conditions are causing excessive rolling / pitching of the barge and / or Own vessel due to which metal to metal contact and damage may result.

· Procedures intended for the operations are inadequate or incorrect 

· Risk assessment is not completed satisfactorily. 


	BEFORE MOORING

	Items
	Checked
	Remarks

	1
	Radio communications, including back-up system, have been agreed and tested and clocks have been synchronized between the ship and the barge
	
	Primary:

Back-up:

	2
	The language of operations has been agreed
	
	Working language: 

	3
	The rendezvous position of the transfer area has been agreed
	
	

	4
	Approach, manoeuvring and mooring plans are understood and confirmed between both parties.
	
	

	5
	Mooring procedures have been agreed, including fender positions and number /type of ropes to be provided by each ship
	
	

	6
	The ships are upright and at a suitable trim, without any overhanging projections on the sides of both vessels.
	
	

	7
	Manoeuvring, mooring and navigational equipment has been tested and found in good order
	
	

	8
	Weather forecasts have been reviewed for the transfer area and arrangements have been made for their continued receipt throughout the operation
	
	

	9
	Weather Condition (Wind direction, speed, Sea, Swell, Precipitation) 
	
	Wind speed / Dir:

Sea:

Swell ht / Dir:

Precipitation:

	10
	The maximum wind and swell criteria for operations have been agreed
	
	Abort approach at:
kts

Stop Transfer at:
kts

Disconnect at:

kts

Cast off at:

kts

	11
	The crew have been briefed on the mooring procedure
	
	

	12
	Local authorities have been advised about the operation
	
	

	13
	The fenders and associated equipment are visually in apparent good order
	
	

	14
	Primary fenders are correctly positioned, and fender rigging is in order
	
	No. of Fenders: 

Size of Fenders:

	15
	Secondary fenders are correctly positioned and secured (Baby fenders)
	
	No. of Fenders: 

Size of Fenders:

	16
	Course and speed information has been exchanged and agreed
	
	

	17
	Adequate lighting is available
	
	

	18
	Power is available for winches and they are in good order
	
	

	19
	Rope messengers, rope stoppers and heaving lines are ready for use
	
	

	20
	All mooring lines are ready
	
	

	21
	Fire axes, or suitable cutting equipment, are in position at the fore and aft mooring stations
	
	

	22
	Crew are standing by at their mooring stations
	
	

	23
	Communications are established with the mooring personnel and bridge. 
	
	

	24
	Fire-fighting and anti-pollution equipment is ready for use
	
	

	25
	Shipping traffic in the area is being monitored
	
	

	26
	The vessel status has been appropriately set on the Automatic Identification System (AIS)
	
	

	27
	Ship’s particulars for the barge have been obtained  
	
	

	28
	Master has a clear understanding that barge should not be allowed to approach or continue operations if he determines that the weather/sea/swell conditions are causing excessive rolling/ pitching and/or the fendering is inadequate and that there is a possibility of hull contact as a result
	
	

	29
	Coir fenders or other portable fenders to be kept standby on own vessel, where available.
	
	

	30
	One responsible officer from ship has been delegated to supervise the mooring operation
	
	

	31
	Engine Staff informed about the side to make fast the barge and manifold requirements.
	
	

	BEFORE UNMOORING

	Items
	Checked
	Remarks

	1
	Barge hoses are properly drained prior to disconnection
	
	

	2
	The transfer side of the ship is clear of obstructions (including hose lifting equipment)
	
	

	3
	The method of letting go mooring and separation of vessels have been agreed and crew have been briefed on procedures
	
	

	4
	Fenders, including fender rigging, are in good order
	
	

	5
	Secondary fenders are correctly positioned and secured for departure
	
	

	6
	Crew are standing by at their mooring stations
	
	

	7
	Communications are established with mooring personnel and with the barge tanker
	
	

	8
	Mooring personnel have been instructed to let go only as directed by the Master
	
	

	Master’s name
	: 
	

	Signature
	:
	

	Date
	:
	



