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	Discharging ship’s name:
	Name of STS Organiser – Superintendent:

	Company
	: 
	
	
	
	

	Call Sign / INMARSAT No
	:
	
	Proposed Date of Transfer
	: 
	

	IMO Number
	:
	
	Proposed Berth / Terminal
	:
	

	Receiving ship’s name
	:
	
	
	
	

	Company
	: 
	
	
	
	

	Call Sign / INMARSAT No
	:
	
	
	
	

	IMO Number
	:
	
	
	
	


	
	Discharge ship Checked
	Receiving Ship Checked
	Terminal / STS organizer Checked

	1
	A standard pre-transfer checklist, such as the ISGOTT ship/shore safety checklist or equivalent, has been satisfactory completed and arrangements have been made for repetitive checks during transfer
	
	
	

	2
	Required regional checklists have been completed
	
	
	

	3
	Written permission for cargo operation to take place are available to all Responsible Persons
	
	
	

	4
	The formal Risk Assessment has been communicated by the transfer organiser and reviewed by involved parties 
	
	
	

	5
	The general contingency plan for the cargo transfer operation has been communicated by the transfer organiser and reviewed by involved parties.
	
	
	

	6
	Security information has been exchanged and, if required, a Declaration of security has been completed.
	
	
	

	7
	Suitable fenders are rigged correctly to prevent contact of the vessels
	
	
	

	8
	Fire axes, or suitable cutting equipment, are in place at the fore and aft mooring stations 
	
	
	

	9
	Present and forecast weather and sea conditions have been considered
	
	
	

	10
	A means of access is in place to allow personnel to safely transit between the vessels
	
	
	

	11
	Cargo specifications and any requirements for inerting, heating, reactivity, and inhibitors have been exchanged
	
	
	

	12
	The cargo transfer operation is to be completed under closed conditions 
	
	
	

	13
	Where applicable, procedures for vapour control/balancing have been agreed
	
	
	

	14
	All cargo monitoring system, including level gauges, high level alarms, pressure gauges and alarms, have been tested and are operational
	
	
	

	15
	Where necessary, permissions for tank cleaning have been obtained and procedures are in place
	
	
	

	16
	Access to the cargo deck is restricted and controlled during cargo transfer operations
	
	
	

	17
	All personnel engaged in the cargo operation are provided with appropriate PPE including, where necessary, personal gas detectors/monitors 
	
	
	

	18
	Cargo hoses have been pressure tested within the prescribed period and documentation is available on board
	
	
	

	19
	The construction and material of the cargo hoses is suitable for the temperature and nature of the product(s)
	
	
	

	20
	Where electrically continuous hoses are used, the hoses are connected to the vessel with the insulated flange before being passed to the other vessel for connection
	
	
	

	21
	The cargo hose sting is of adequate length and properly supported
	
	
	

	22
	The cargo lines are lined up in accordance with the cargo operation plan
	
	
	

	23
	Spill response equipment is on station and ready for immediate deployment
	
	
	

	24
	Where applicable, fire-fighting provision has been made for unmanned barges
	
	
	

	25
	Spaces to be routinely monitored for any build-up of flammable and/or toxic vapour have been identified
	
	
	

	
	Signature:
	Name:

	Officer in Charge Discharging Ship:
	
	

	Officer in Charge Receiving Ship:
	
	

	Terminal:
	
	

	STS Superintendent / STS organizer:
	
	



