



SAF 03 – Risk Assessment 


	Risk Management

	Operation / Work activity being assessed:
	INSPECTION / MAINTENANCE OF HIGH VELOCITY P/V VALVE OF COT.

	
	 FORMCHECKBOX 
 Routine        FORMCHECKBOX 
 Non-routine

	Generated by: Vessel  FORMCHECKBOX 
 (record the name)
	 FORMCHECKBOX 
Office

	Code number (to be assigned by the Office): 1.65  


	FREQUENCY CATEGORY
	
	CONSEQUENCE CATEGORY
	
	RISK MATRIX

	5
	Frequent - Possibility of repeated incidents
	More often than once per voyage
	
	4
	Human losses / fatalities
	Major pollution / 

Full scale response
	Excessive/ high cost damage >$1000000
	Major national &  international impact
	
	
	FREQUENCY

	4
	Probable - Possibility of isolated incidents
	Once per  year
	
	3
	Serious injury to personnel
	Moderate pollution/ 

Significant resources  commitment
	Moderate  cost or damage 

(100000 –1000000$)
	Considerable impact
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	1
	2
	3
	4
	5

	3
	Occasional- Possibility of occurring sometime
	Once per 5 years
	
	2
	Number of minor injuries /  Medical treatment for personnel
	Little pollution / 

Limited response of short duration
	Little cost or damage 

($10000 – $ 100000)
	Slight impact
	
	CONSEQUENCE
	1
	L(1)
	L(2)
	L(3)
	M(4)
	M(5)

	
	
	
	
	
	
	
	
	
	
	
	2
	L(2)
	M(4)
	M(6)
	M(8)
	H(10)

	2
	Remote- Not likely to occur
	Once per 10 years
	
	1
	Few minor injuries
	Minimum pollution /

Little or no response needed
	Minimum cost / damage 

< $10000
	Zero impact
	
	
	3
	L(3)
	M(6)
	M(9)
	H(12)
	H(15)

	1
	Very unlikely- Practically impossible
	Once per  30 years or more
	
	
	
	
	
	
	
	
	4


	M(4)
	M(8)
	H(12)
	H(16)
	H(20)

	
	
	
	
	
	
	
	
	
	
	High=Intolerable Risk   Medium=Tolerable Risk    Low=Acceptable Risk


	Risk Assessment

	
	Risk Identification
	Risk Analysis
	Initial risk evaluation

	No
	Hazard
	Potential

hazardous event
	Existing control measures
	F
	C
	R

	1
	Injury from tools.
	Number of minor injuries
	Experienced crew members will be involved with appropriate P.P.E.
	3
	2
	6

	2
	Vent pipe under pressure.
	·    Serious injury to personnel 

· Moderate cost or damage 
	The vent pipe is drained and vented to atmosphere.
	4
	3
	12

	3
	Inhalation of toxic gasses.
	· Fatality

· Moderate pollution 
	Atmosphere test carried out prior commencement of work.
	4
	4
	16

	4
	Damage of the valve sealing.
	Moderate cost or damage
	Experienced crew will be involved.
	4
	3
	12

	Note F: Frequency, C: Consequence, R: Risk


	Risk Treatment
	Residual risk evaluation

	Hazard No.
	Additional Risk Control Measures
	Responsible
	Action Timeline 
	F
	C
	R

	1
	Experienced crew members will carry out the work. Gears, rigging to be used are in good condition. Safety harnesses and belts with life lines are provided.
	C/E
	Before task
	1
	3
	3

	2
	COT depressurized and vent pipe vented to atmosphere.
	C/E
	During task
	1
	3
	3

	3
	COT depressurized and vent pipe vented to atmosphere.
	C/E
	During task
	1
	4
	4

	4
	Valves must be handled with caution.
	C/E
	During task
	1
	3
	3

	Note F: Frequency, C: Consequence, R: Risk


	ALTERNATIVE WAYS TO CONDUCT THE WORK (a new RA should be conducted for the alternative way decided)

	


	Are any amendments to IMS required (related to the above Additional Risk Control Measures)?

	Yes  FORMCHECKBOX 
  Describe:

	No    FORMCHECKBOX 



	Contingency plans (to facilitate safe management and recovery of the situation in case of any unplanned occurrences)

	Emergency case
	Contingency Plans

	DECK EQUIPMENT FAILURE
	REFER TO COMPANY’S SHIP EMERGENCIES.


	Risk Management Team

	Name
	Rank / Title
	Signature
	Date

	
	
	
	

	
	
	
	

	
	
	
	

	Remarks:


	Risk Assessment reviewed/approved by:

	Name
	Rank / Title
	Signature
	Date

	
	
	
	

	
	
	
	

	Remarks:
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