









SAF 03 – Risk Assessment 


	Risk Management

	Operation / Work activity being assessed:
	BUNKERING DURING HEAVY WEATHER

	
	 FORMCHECKBOX 
 Routine        FORMCHECKBOX 
 Non-routine

	Generated by: Vessel  FORMCHECKBOX 
 (record the name)
	 FORMCHECKBOX 
Office

	Code number (to be assigned by the Office): 2.20  


	FREQUENCY CATEGORY
	
	CONSEQUENCE CATEGORY
	
	RISK MATRIX

	5
	Frequent - Possibility of repeated incidents
	More often than once per voyage
	
	4
	Human losses / fatalities
	Major pollution / 

Full scale response
	Excessive/ high cost damage >$1000000
	Major national &  international impact
	
	
	FREQUENCY

	4
	Probable - Possibility of isolated incidents
	Once per  year
	
	3
	Serious injury to personnel
	Moderate pollution/ 

Significant resources  commitment
	Moderate  cost or damage 

(100000 –1000000$)
	Considerable impact
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	1
	2
	3
	4
	5

	3
	Occasional- Possibility of occurring sometime
	Once per 5 years
	
	2
	Number of minor injuries /  Medical treatment for personnel
	Little pollution / 

Limited response of short duration
	Little cost or damage 

($10000 – $ 100000)
	Slight impact
	
	CONSEQUENCE
	1
	L(1)
	L(2)
	L(3)
	M(4)
	M(5)

	
	
	
	
	
	
	
	
	
	
	
	2
	L(2)
	M(4)
	M(6)
	M(8)
	H(10)

	2
	Remote- Not likely to occur
	Once per 10 years
	
	1
	Few minor injuries
	Minimum pollution /

Little or no response needed
	Minimum cost / damage 

< $10000
	Zero impact
	
	
	3
	L(3)
	M(6)
	M(9)
	H(12)
	H(15)

	1
	Very unlikely- Practically impossible
	Once per  30 years or more
	
	
	
	
	
	
	
	
	4


	M(4)
	M(8)
	H(12)
	H(16)
	H(20)

	
	
	
	
	
	
	
	
	
	
	High=Intolerable Risk   Medium=Tolerable Risk    Low=Acceptable Risk


	Risk Assessment

	
	Risk Identification
	Risk Analysis
	Initial risk evaluation

	No
	Hazard
	Potential

hazardous event
	Existing control measures
	F
	C
	R

	1
	During bunkering, the mooring ropes holding the bunker barge broke due to bad weather resulting detach of the barge, breaking of the bunkering pipe and eventually polluting.
	· Moderate  cost or damage 

· Moderate pollution/  Significant resources  commitment
	· Safety Management System 

· ISGOTT V-§ 2.7, 4.1, 22.2, 25.2, 25.4.
· C.O.S.W.P. ( M.C.A) Reference Section 30.2 (Carrying Bulk Liquid Cargoes).
	4
	3
	12

	Note F: Frequency, C: Consequence, R: Risk


	Risk Treatment
	Residual risk evaluation

	Hazard No.
	Additional Risk Control Measures
	Responsible
	Action Timeline 
	F
	C
	R

	1
	A. Bunkering in adverse weather conditions should be avoided. Extra care should be taken if necessary to proceed in bunkering during adverse weather conditions.
	C/O / C/E
	Before and during bunkering
	2
	3
	6

	
	B. Additional mooring lines to be added when bunkering during bad weather.
	Master / C/O
	Before and during bunkering
	
	
	

	
	C. Rest hours of all involved personnel to be considered.
	Master / C/E
	Before bunkering
	
	
	

	Note F: Frequency, C: Consequence, R: Risk


	ALTERNATIVE WAYS TO CONDUCT THE WORK (a new RA should be conducted for the alternative way decided)

	


	Are any amendments to IMS required (related to the above Additional Risk Control Measures)?

	Yes  FORMCHECKBOX 
  Describe:

	No    FORMCHECKBOX 



	Contingency plans (to facilitate safe management and recovery of the situation in case of any unplanned occurrences)

	Emergency case
	Contingency Plans

	FIRE, EXPLOSION
	REFER TO COMPANY’S SHIP EMERGENCIES (FIRE).


	Risk Management Team

	Name
	Rank / Title
	Signature
	Date

	
	
	
	

	
	
	
	

	
	
	
	

	Remarks:


	Risk Assessment reviewed/approved by:

	Name
	Rank / Title
	Signature
	Date

	
	
	
	

	
	
	
	

	Remarks:
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