



SAF 03 – Risk Assessment 


	Risk Management

	Operation / Work activity being assessed:
	FOULING THE PROPELLER DURING UNBERTHING MANOEUVRES

	
	 FORMCHECKBOX 
 Routine        FORMCHECKBOX 
 Non-routine

	Generated by: Vessel  FORMCHECKBOX 
 (record the name)
	 FORMCHECKBOX 
Office

	Code number (to be assigned by the Office): 8.12  


	FREQUENCY CATEGORY
	
	CONSEQUENCE CATEGORY
	
	RISK MATRIX

	5
	Frequent - Possibility of repeated incidents
	More often than once per voyage
	
	4
	Human losses / fatalities
	Major pollution / 

Full scale response
	Excessive/ high cost damage >$1000000
	Major national &  international impact
	
	
	FREQUENCY

	4
	Probable - Possibility of isolated incidents
	Once per  year
	
	3
	Serious injury to personnel
	Moderate pollution/ 

Significant resources  commitment
	Moderate  cost or damage 

(100000 –1000000$)
	Considerable impact
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	1
	2
	3
	4
	5

	3
	Occasional- Possibility of occurring sometime
	Once per 5 years
	
	2
	Number of minor injuries /  Medical treatment for personnel
	Little pollution / 

Limited response of short duration
	Little cost or damage 

($10000 – $ 100000)
	Slight impact
	
	CONSEQUENCE
	1
	L(1)
	L(2)
	L(3)
	M(4)
	M(5)

	
	
	
	
	
	
	
	
	
	
	
	2
	L(2)
	M(4)
	M(6)
	M(8)
	H(10)

	2
	Remote- Not likely to occur
	Once per 10 years
	
	1
	Few minor injuries
	Minimum pollution /

Little or no response needed
	Minimum cost / damage 

< $10000
	Zero impact
	
	
	3
	L(3)
	M(6)
	M(9)
	H(12)
	H(15)

	1
	Very unlikely- Practically impossible
	Once per  30 years or more
	
	
	
	
	
	
	
	
	4


	M(4)
	M(8)
	H(12)
	H(16)
	H(20)

	
	
	
	
	
	
	
	
	
	
	High=Intolerable Risk   Medium=Tolerable Risk    Low=Acceptable Risk


	Risk Assessment

	
	Risk Identification
	Risk Analysis
	Initial risk evaluation

	No
	Hazard
	Potential

hazardous event
	Existing control measures
	F
	C
	R

	1
	During unberthing manoeuvres from SBM, floating terminal hose became entangle with propeller causing engine to stop and subsequent damage to propeller seal.
	Moderate  cost or damage


	Safety Management Procedures
	3
	4
	12

	Note F: Frequency, C: Consequence, R: Risk


	Risk Treatment
	Residual risk evaluation

	Hazard No.
	Additional Risk Control Measures
	Responsible
	Action Timeline 
	F
	C
	R

	1
	A. There must be supervision through the operation.
	Officer on duty
	During operation
	1
	4
	4

	
	B. The officer in charge of the mooring operation must oversee the entire operation without getting involved in any other tasks.
	Officer on duty
	During operation
	
	
	

	
	C. The Deck Officer in charge should ensure anchors readiness during sailing from berth. Due adjustment to the above procedure should be made in case of specific local requirements. 
	Deck Officer in charge
	Prior to operation
	
	
	

	
	D. The Deck Officer in charge at the aft mooring stations should pay attention to keeping the propeller clear, informing the bridge accordingly.
	Deck Officer in charge
	During

operation
	
	
	

	
	E. Prior to any ship’s movement it should be ensured that mooring lines are clear of any jetty fittings/obstructions thus avoiding a line being entangled / damaged.
	Master /

Deck Officer in charge
	Prior to operation
	
	
	

	Note F: Frequency, C: Consequence, R: Risk


	ALTERNATIVE WAYS TO CONDUCT THE WORK (a new RA should be conducted for the alternative way decided)

	


	Are any amendments to IMS required (related to the above Additional Risk Control Measures)?

	Yes  FORMCHECKBOX 
  Describe:

	No    FORMCHECKBOX 



	Contingency plans (to facilitate safe management and recovery of the situation in case of any unplanned occurrences)

	Emergency case
	Contingency Plans

	GROUNDING, DANGEROUS STRUCTURAL DAMAGE
	REFER TO COMPANY’S SHIP EMERGENCIES (HULL FAILURE, GROUNDING OR STRANDING).


	Risk Management Team

	Name
	Rank / Title
	Signature
	Date

	
	
	
	

	
	
	
	

	
	
	
	

	Remarks:


	Risk Assessment reviewed/approved by:

	Name
	Rank / Title
	Signature
	Date

	
	
	
	

	
	
	
	

	Remarks:
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