S4 – NON-RESTRICTED AREAS WITH ADDITIONAL SECURITY

Ship’s Name:


	This table is to be completed for areas which are not defined as restricted but which the SSO or Master considers should have a degree of added security attached. 

	Description
	Location
	SECURITY STATE AND KEY HOLDER
	Remarks

	Lifeboats
	
	Enclosed. To be sealed with plastic seals when in port, check during deck patrols.
	

	 Bunker Manifolds 
	
	To be continuously monitored in port and also during cable operation, Bunker operations, checked during patrols.
	

	Oil spill locker
	
	May be sealed with plastic seals when in port and not in use; checked during deck patrols. If padlocked the key must be easily accessible in emergency.
	Do not lock when bunkering.

	Fresh Water Filling Pipes
	
	To be monitored during receiving fresh water and check for tampering during deck patrols.
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