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CCR 53: Deck Seal Inspection
Deck Seal should be checked at least every 3 months and should be clean. The Observation Glass should be cleaned as required.
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