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	Vessel Name:
	Name of port/berth:

	Description of work:   
	Location of work:

	This permit is valid from
	:
	
	Hrs LT
	Date:

	(Maximum validity 8 hours)
to
	:
	
	Hrs LT
	Date:

	Remarks:

· Refer to FOM 10.13 Section 4.6 “Diving / Underwater operations” in conjunction with this permit.

· In case there are any changes in the conditions impacting the diving operation or the blanking arrangement (example weather conditions etc.), risk assessment and control measures should be reviewed, and appropriate measures enforced.


	Description
	Yes
	NA
	Description
	Yes
	N/A

	Risk assessment, daily safety meeting and onsite toolbox meeting carried out.
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Flag “A” / RAM light displayed 
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Pre-diving safety conference held
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Trim / draft /list adjusted if required
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Other necessary permits issued: (Consider Coldwork Permit – HSSEQ-08 /  Small Craft Alongside Permit – HSSEQ-36) 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Method of blanking agreed *
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Weather/sea conditions suitable
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Bilge pumps / Emergency Bilge Pump lined up
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Relevant personnel (OOW / Duty engineer / other crew) informed
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Inboard blank flanges prepared
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Contingency measures established (in case blanking arrangement fails)
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Arrangements for diving craft to stay alongside during operations are in place
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Communications protocol agreed with diving team and tested
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Emergency communication medium (e.g. VHF, Shore phone etc.) confirmed
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	English being agreed as language of communication with the diving team
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Anchors secured
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Experienced/Trained and adequate crew available for the task
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	ME / Propeller / thrusters isolated
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Safety observer appointed 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Steering gear isolated
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Adequate illumination provided
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	G/E cooling discharge minimum
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Safe access/egress provided
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	A/C plant operation ceased
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Permission obtained from port authority/terminal supervisor
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Speed log/echo sounder switched off
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Cautionary notices posted 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	ICCP switched off and secured
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Ladder/gangway kept in readiness
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	All overboard discharges shut
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Work area clear of cargo operations
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Applicable sea intakes shut
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	No other vessels alongside
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Applicable pumps isolated
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	No cargo/ballast/storing operations in progress
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Applicable valves closed/lashed
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	No other work interfering the operations
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Siting of diving equipment safe
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Lifebuoy with line available
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Lockout/Tagout:HSSEQ-34 completed 
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Rescue boat/Fast rescue boat/Terminal boat in readiness
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Valve diagrams explained to diving team
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Emergency Response Plan agreed
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Vessels in vicinity informed
	 FORMCHECKBOX 

	 FORMCHECKBOX 


	Is office informed where applicable 
	 FORMCHECKBOX 

	 FORMCHECKBOX 

	Critical Maintenance Permit & Office Concurrence Form E30 completed
	 FORMCHECKBOX 

	 FORMCHECKBOX 



	Any special conditions/precautions:


	The above mentioned points have been checked and the conditions at the site, or of the equipment to be worked on, are safe for the work to be undertaken

	Rank
	Signature
	Date / time
	Rank
	Signature
	Date / time

	Responsible officer
	
	
	Diving company supervisor
	
	

	Master
	
	
	
	
	


	PERMIT TO WORK CANCELLED (If prior to job completion, give reasons):



	Completion of job (To be completed by the responsible person) 

The work has been completed and all persons under my supervision, materials and equipment have been withdrawn. All items re-secured and lock / tag out removed. The work area and equipment has been left in a safe condition. All persons involved advised and permit has ended.



	Rank
	Name
	Date / time
	Signature

	Responsible officer
	
	
	

	Note: This permit is rendered invalid if any of the conditions noted in the checklist change

	* Refer to FOM 10.11 “Standard under water blanking arrangements” & FOM 10.13 Section 4.6.1 - Underwater Blanking Operations by divers.



