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	Vessel
	:
	

	Note: Log down the position from BOTH the GPS once a watch for comparison and mention such comparison in remarks column. 
On the occasions, position from ANY ONE GPS shall suffice the requirement.

Alternate means of position fixing – bearing and distance from fixed landmark, etc. to be exercised (whenever applicable) during the passage.

	Date
	Time

LT
	Time

UTC
	GPS 1
	GPS 2
	XTE
	DTG to   WPT
	Total DTG
	Course
	Speed
	(A) Ship’s Draft at Transducer (m)
	(B) UKC as per Echo Sounder
	(A+B)

Depth as per Echo Sounder
	Chart Depth
	Alternate Position Fixing/Verification - Bearing and distance (Fixed Landmarks, buoys, etc)
	Signature of OOW
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	Long
	Lat
	Long
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CC*: Chartered Course; SC*: Steered Course; GS*: GPS Speed; LS*: Log Speed

· Signal to noise ratio (SNR): A ratio of 10-15dB is the accepted minimum to establish an unreliable connection; 16-24 dB is usually considered poor; 25-40 is good and a ratio of 41dB or higher is considered excellent.

· Dilution of Precision (PDOP/HDOP): The PDOP values should be in range of 6.0 or less. HDOP values should be in range of 4.0 or less. Inform Master in case the values are higher than recommended. 
· Ensure that the GPS is not on DR mode. 
                                                                                                                                                                                                                                                                Master
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